**ALGORITHM:**

[1] start

[2] Initialize all the modules

[3] check input from GSM

If msg == vote A

Then increment vote A count and

Display on LCD

Else if msg == vote B

Then increment vote B count and

Display on LCD

Else if msg == vote C

Then increment vote C count and

Display on LCD

Else if msg == vote D

Then increment vote D count and

Display on LCD

Else

Invalid contains

Then buzzer will ON

Otherwise it remains OFF

[4] go to step (2)